

**Composition of gases obtained from pyrolysis of HDPE at 150 0C and 250 0C with spent FCC catalyst using catalyst/sample ratio of 1:8**



**Composition of gases obtained from pyrolysis of HDPE at 150 0C and 250 0C with spent FCC catalyst using catalyst/sample ratio of 1:16**